**GM6S监视器固件说明中英文**

**GM6S Monitor Firmware User Guide**

一、请从神牛官网下载监视器固件，把压缩文件解压到SD卡根目录下，完成后把卡插入监视器卡槽，从菜单→设置→升级→升级→确认，等待约3分钟完成升级后即可。

二、版本号查看方法：菜单→设置→升级

三、版本说明：

1. Download the firmware for the monitor on [www.godox.com,](http://www.godox.com,) unzip the firmware to the root directory of the SD card, and insert SD card into the monitor card slot, then enter into the monitor’s Menu→Setting→Upgrade→Upgrade→Confirm, after that approx. 3 minutes will take to complete the upgrade.

2. Firmware version checking steps: Menu→Setting→Upgrade

3. Firmware version introduction is followed:

|  |  |  |
| --- | --- | --- |
| **版本 Version** | **更新内容 Upgraded Content** | **日期 Date** |
| B1.1.97 | 1. 优化相机控制菜单触摸识别   Optimize camera control menu touch recognition   1. 拍照、录像、自动对焦添加到F键选项中   Add photo, video and auto focus to the F key options | 2022-08-19 |
| B1.2.01 | 更新UI，触摸相机控制菜单区域图标有动态提示 Update UI, touch camera control menu area icon has dynamic prompt | 2022-09-24 |
| V1.2.42 | 1.遮幅区域新增两个选项  Two new options added to the masking area 2.支持辅助调焦和斑马纹功能同时打开 Supports simultaneous activation of auxiliary focus and zebra pattern functions | 2025-03-07 |
|  |  |  |
|  |  |  |

**注：详细规格请在官网（www.godox.com）下载最新说明书。**

**Note: For more details, please download the latest user manual from the official website (www.godox.com).**